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	Safe crane operation - Risk assessment before starting work /LMRA/

	Name of Company:
	
	
Work permit number:

	

	The crane process can only be started and the related WORK PERMIT is only valid if the people performing the work, under the guidance of the on-site work supervisor, have thought through the task before them, assessed the conditions and dangers of the work site and based on these, have answered "X" to the to the following (I-yes, N-no, Nv-no applies):

	No.
	Statement
	Y
	N
	NN  N.
 A.

	No.
	Statement
	Y
	N
	NN  N.
A.


	1.
	The lifting machine to be used received the appropriate qualification as documented during the operator check before starting work according to the Lifting Machine Safety Regulations.
	
	
	
	11.
	The lifting machine used to carry out the work, the load lifting and suspension devices have valid documents and periodic inspections.

	
	
	

	2.
	The lifting machine operator is entitled to operate the given lifting machine and has a valid medical qualification and mandate.
	
	
	
	12.
	We have read and understood the contents of the work permit, and we will keep them during the work.
	
	
	

	3.
	The person assigned to tie the load is authorized and authorized to perform the given work.
	
	
	
	13.
	We clarified the time process of the work, as well as the role of each employee in performing the work.
	
	
	

	4.
	The operator (controller) assigned to manage the lift received an order for this task from the operator.
	
	
	
	14.
	We are qualified and trained to handle our work tools in a condition suitable for carrying out the work.
	
	
	

	5.
	The available location is sufficient for setting up the lifting machine, safely picking up, moving, and putting down the load.
	
	
	
	15.
	We know what to do in an emergency (accident, fire, explosion), escape routes, and know how to call for help.
	
	
	

	6.
	The load-bearing capacity of the surface required for footing corresponds to the largest transfer load expected during lifting.
	
	
	
	16.
	Our work environment is suitable for work, which we keep clean and tidy during work.

	
	
	

	7.
	The lifting machine, the load handler, the suspension device are suitable for the weight and/or design and size of the load to be moved.
	
	
	
	17.
	All hazardous energy sources and external conditions have been treated in the prescribed manner, which do not pose any further danger.
	
	
	

	8.
	The load capacity of the suspension device per branch is suitable for carrying out the lifting even in the case of the largest expected angle enclosed by the rope branches.
	
	
	
	18.
	By closing the dangerous area, fencing it off and/or appointing a watcher, we have taken care of eliminating the danger from falling objects.
	
	
	

	9.
	If a person is lifted, all personal and material conditions are provided - including the full body harness.
	
	
	
	19.
	Everyone wears the necessary and prescribed protective equipment, they are undamaged and suitable for use.
	
	
	

	10.
	If the use of an individual rescue (self-rescue) device is mandatory, the self-rescue device is in the personnel carrier and is operational.
	
	
	
	20.
	We work carefully, we do not endanger others, and we do not condone unsafe work around us.
	
	
	

	
Lifting machine operator
	Name (printed)
	Signature
	Date / Time

	
	
	
	 
year        month       day       hour        min

	Designated controller person
	Name (printed)
	Signature
	Date / Time

	
	
	
	 
year        month       day       hour        min

	The binders participating in the work, auxiliary force

	Name (printed)
	Signature
	Date / Time

	
	

	
	      
year        month       day       hour        min



	
	
	
	
year        month       day       hour        min


	
	
	
	
year        month       day       hour        min
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